| Routines

92BA: Print a message

Used by the routines at 85CC, 8684, 870E, 8944 and 9028.
Input
IX | Address of the message
C | Length of the message
DE | Display file address
92BA | LD A,(IX+$00) | Collect a character from the message
92BD | CALL $92CB | Print it
92C0 | INC IX | Point IX at the next character in the message
92C2 | INC E | Point DE at the next character cell (subtracting 8 from D compensates for the operations performed by the routine at 92CB)
92C3 | LD A,D
92C4 | SUB $08
92C6 | LD D,A
92C7 | DEC C | Have we printed the entire message yet?
92C8 | JR NZ,$92BA | If not, jump back to print the next character
92CA | RET |