| Routines

9680: Print a message

Used by the routines at 86C3, 87CA, 8912, 89AD and 8C4A.
Input
IX | Address of the message
C | Length of the message
DE | Display file address
9680 | LD A,(IX+$00) | Collect a character from the message
9683 | CALL $9691 | Print it
9686 | INC IX | Point IX at the next character in the message
9688 | INC E | Point DE at the next character cell (subtracting 8 from D compensates for the operations performed by the routine at 9691)
9689 | LD A,D
968A | SUB $08
968C | LD D,A
968D | DEC C | Have we printed the entire message yet?
968E | JR NZ,$9680 | If not, jump back to print the next character
9690 | RET |